AUTOMATIC TRANSMISSION • VALVE BODY LAB
VALVE BODY DISASSEMBLY
Component Location & Check-Off Task Sheet
	Name
	____________________________
	Date
	______________

	Team / Bay
	____________________________
	Instructor
	______________


TASK
Carefully disassemble the valve body. Use the exploded view to identify each component, place it in order, and check it off on page 2.
1. Set the valve body on a clean tray and compare its orientation to the diagram.
2. Remove one bore assembly at a time. Keep every valve, spring, plug, and retainer in removal order.
3. Match each part to its reference number and component name on page 2.
4. Do not mix similar-looking valves or springs. Ask the instructor before forcing or prying any component.
5. Complete the final inspection and obtain instructor initials before reassembly.
EXPLODED VIEW — USE THE REFERENCE NUMBERS TO IDENTIFY PARTS
[image: ]
COMPONENT LOCATION CHECKLIST
Check each box only after the component has been removed, identified, and placed in the correct order.
	Check
	Ref.
	Component
	Check
	Ref.
	Component

	☐
	340
	Valve, Manual
	☐
	373
	Plug, Bore

	☐
	350
	Valve Assembly, Control Body
	☐
	374
	Valve, Actuator Feed Limit

	☐
	353
	Seal, Forward Accumulator Oil
	☐
	375
	Spring, Actuator Feed Limit Valve

	☐
	354
	Piston, Forward Accumulator
	☐
	376
	Plug, Bore

	☐
	355
	Pin, Forward Accumulator
	☐
	377
	Pressure Control Solenoid

	☐
	356
	Spring, Forward Accumulator
	☐
	378
	Retainer, Pressure Control Solenoid

	☐
	357
	Valve, Forward Abuse
	☐
	379
	Retainer, Solenoid

	☐
	358
	Spring, Forward Abuse Valve
	☐
	380
	Valve, Converter Clutch Signal

	☐
	359
	Plug, Bore
	☐
	381
	Plug, Bore

	☐
	360
	Pin, Coiled Spring
	☐
	382
	Spring, 4–3 Sequence Valve

	☐
	361
	Valve, Low Overrun
	☐
	383
	Valve, 4–3 Sequence

	☐
	362
	Spring, Low Overrun Valve
	☐
	384
	Valve, 3–4 Relay

	☐
	363
	Cover, Forward Accumulator
	☐
	385
	Valve, 3–4 Shift

	☐
	364
	Bolt, Forward Accumulator Cover
	☐
	386
	Spring, 3–4 Shift Valve

	☐
	365
	Spring, 1–2 Shift Valve
	☐
	387
	Valve, Reverse Abuse

	☐
	366
	Valve, 1–2 Shift
	☐
	388
	Spring, Reverse Abuse Valve

	☐
	367A
	Shift Solenoid A (1–2–3–4)
	☐
	389
	Valve, 3–2 Downshift

	☐
	367B
	Shift Solenoid B (2–3)
	☐
	390
	Spring, 3–2 Downshift Valve

	☐
	368
	Valve, 2–3 Shift
	☐
	391
	Valve, 3–2 Control

	☐
	369
	Valve, 2–3 Shuttle
	☐
	392
	Spring, 3–2 Control Valve

	☐
	370
	Spring, Accumulator Valve
	☐
	393
	Spring, Bore Plug

	☐
	371
	Valve, Accumulator
	☐
	394
	3–2 Control Solenoid

	☐
	372
	Sleeve, Accumulator Valve
	☐
	395
	Retainer, Bore Plug


FINAL INSPECTION
☐ All listed components were located and identified.
☐ Parts are arranged in correct removal order.
☐ No components are damaged, missing, or mixed with another group.
Instructor Initials: ____________________     Completion:  ☐ Satisfactory   ☐ Needs Review
Handle all valves, plugs, springs, retainers, and solenoids carefully. Do not force parts.
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